DAQ Workplan:

Introduction

Timescale:

need something for ROD – 6 months prototype of final DAQ – 18 months

Minimal configuration for ROD tests: n * DSS n * ROD TCM or TTCvi VICs?

possibly other phase II modules?

DAQ Evolution: Use of

Atlas DAQ-1

Try moving existing DAQ code to Linux – NB only draft real time Posix code? VME Access: PCI-VME interface (or net+Lynx) Try replacing EMU with MRS/IS Design database:

– configuration: crates, modules – parameters: run type, modules, etc Implement & populate database with OKS Provide GUI to dynamically control DB... Run Control (RC) skeleton for daqprod etc Provide C++ objects for ROD, DSS, TTCvi... Use these to write new daqprod Same event format ⇒ still use daqana?

Software Workplan

New DAQ for ROD and other prototypes – 6–18 months New diagnostics: agree with Cornelius – 6–18 months Both should use same low level code? Calibration software – 18 months?

Monitoring software – 18 months?