Rack Layout 1 Murrough Landon

Rack Layout

Murrough Landon – 28 June 2001

http://www.hep.ph.qmw.ac.uk/~landon/talks

Why revisit this now?

• Tentative layouts around for some time • Now pressure from Chris Parkman to enter information into his database:

– Which crates are in which racks – Estimated power consumption:

Receivers, PP, CP, JEP, ROD, TTC

Changes since original layout

• Cables will be laid without connectors. So we will only need two holes in the shielding wall, not three • Number (and layout?) of holes has changed – but we dont have the details yet • CTP and TTC are off centre on the floor below

New proposal

• New suggested rack layout:

– Shift trigger racks to one side – Easier access to most crates – CP and JEP above CTP – Use two shielding wall holes (centre and side) • Still need to decide cabling and layout between receivers and preprocessors • Still subject to global optimisation of level 1 trigger latency

L1 Joint Meeting 28 June 2001 Mainz

Rack Layout 2 Murrough Landon

L1 Joint Meeting 28 June 2001 Mainz