Racks

Murrough Landon – 8 November 2001

http://www.hep.ph.qmul.ac.uk/~landon/talks

Overview

• Developments since Mainz • Information given to Chris Parkman • Outstanding issues

Developments since Mainz

Not much!

• The wall really is a wall!

• Layout proposed at Mainz given to Chris Parkman • No changes to my diagrams...

• ...but Bill Cleland wants an extra rack for signal monitoring equipment

Information given to Chris Parkman (1)

Racks

• New layout of racks (still subject to change) – 1 run of 14 racks: all used by calo trigger – 1 run of 9 racks: two used by calo trigger, remainder still reserved for level 1 • Contents of each rack: crates, cabling, etc – 8 Receiver/PP racks: 2 9U crates + 10U for cabling – 1 rack reserved for possible extra TileCal receivers – 3 CP/JEP racks: 2 9U crates + reserved 1 6U crate – 1 TTC/ROD rack: 2 9U crates + 1 6U crate – 1 rack for computers, network switch, etc

Information given to Chris Parkman (2)

Cables

• No further information on cables provided yet • Chris wants to know details about all our cables: type of cable, number of cables, expected route, etc • LAr signals cables are in his database • But no information yet on TileCal cables • And no information yet on internal cables in USA15 • We probably need to reserved underfloor cable trays • We now want to use the central and one side hole through the sheilding wall. But centre hole currently foreseen for the magnet cables.

Outstanding Issues

Racks

• Layout of PP and receiver crates?

• Do we need more than two TileCal receiver crates?

Cables

• Need to move on TileCal cables!

• Internal USA15 cable lengths and latency calculations depend on chosen layout for receiver and PP systems